PV_RectComb make gaps in spectrum

PV_RectComb(buffer, numTeeth, phase, width)

Makes a series of gaps in a spectrum.

buffer - fft buffer.

numTeeth - number of teeth in the comb.

phase - starting phase of comb pulse.

width - pulse width of comb.

See also FFT Overview.

s.boot;

(

{

var in, chain;

in = WhiteNoise.ar(0.2);

chain = FFT(LocalBuf(2048), in);

chain = PV_RectComb(chain, 8, LFTri.kr(0.097, 0, 0.4, 0.5),

LFTri.kr(0.24, 0, -0.5, 0.5));

IFFT(chain).dup;

}.play;

)

(

{ var in, chain;

in = WhiteNoise.ar(0.2);

chain = FFT(LocalBuf(2048), in);

chain = PV_RectComb(chain, MouseX.kr(0, 32), MouseY.kr, 0.2);

IFFT(chain).dup;

}.play;

)