Balance2 stereo signal balancer

Balance2.ar(left, right, pos, level)

Equal power panning balances two channels; by panning, you are favouring one or other channel in the mix, and the other loses power. The middle pan position (pos=0.0) corresponds to the original stereo mix; full left (pos of -1) is essentially just left channel playing, full right (pos of 1) just the right. The output of Balance2 remains a stereo signal.

left - channel 1 of input stereo signal

right - channel 2 of input stereo signal

pos - pan position, -1 is left, +1 is right

level - a control rate level input.

{Balance2.ar(LFSaw.ar(44),Pulse.ar(33),FSinOsc.kr(0.5), 0.1) }.play;

{var source; source= SinOsc.ar([440,550]); Balance2.ar(source[0],source[1],LFNoise0.kr(4),0.3) }.play;