SOS second order filter section (biquad)

Inherits from: Object : AbstractFunction : UGen : Filter

SOS.ar(in, a0, a1, a2, b1, b2, mul, add)

SOS.kr(in, a0, a1, a2, b1, b2, mul, add)

A standard second order filter section. Filter coefficients are given directly rather than calculated for you.

Formula is equivalent to:

out(i) = (a0 * in(i)) + (a1 * in(i-1)) + (a2 * in(i-2))

+ (b1 * out(i-1)) + (b2 * out(i-2))

// example: same as TwoPole

(

{

var rho, theta, b1, b2;

theta = MouseX.kr(0.2pi, pi);

rho = MouseY.kr(0.6, 0.99);

b1 = 2.0 * rho * cos(theta);

b2 = rho.squared.neg;

SOS.ar(LFSaw.ar(200, 0, 0.1), 1.0, 0.0, 0.0, b1, b2)

}.play

)

(

{

var rho, theta, b1, b2;

theta = MouseX.kr(0.2pi, pi);

rho = MouseY.kr(0.6, 0.99);

b1 = 2.0 * rho * cos(theta);

b2 = rho.squared.neg;

SOS.ar(WhiteNoise.ar(0.1 ! 2), 1.0, 0.0, 0.0, b1, b2)

}.play

)

// example with SOS.kr kr as modulator

(

{

var rho, theta, b1, b2, vib;

theta = MouseX.kr(0.2pi, pi);

rho = MouseY.kr(0.6, 0.99);

b1 = 2.0 * rho * cos(theta);

b2 = rho.squared.neg;

vib = SOS.kr(LFSaw.kr(3.16), 1.0, 0.0, 0.0, b1, b2);

SinOsc.ar( vib * 200 + 600) * 0.2

}.play

)