Lag exponential lag

Lag.ar(in, lagTime, mul, add)

Lag.kr(in, lagTime, mul, add)

This is essentially the same as OnePole except that instead of supplying the coefficient directly, it is calculated from a 60 dB lag time. This is the time required for the filter to converge to within 0.01 % of a value. This is useful for smoothing out control signals.

in - input signal

lagTime - 60 dB lag time in seconds.
See also LagUD, Ramp

(

// used to lag pitch

{

SinOsc.ar( // sine wave

Lag.kr( // lag the modulator

LFPulse.kr(4, 0, 0.5, 50, 400), // frequency modulator

Line.kr(0, 1, 15) // modulate lag time

),

0, // phase

0.3 // sine amplitude

)

}.play

)