BufDelayC buffer based simple delay line with cubic interpolation

BufDelayC.ar(buf, in, delaytime, mul, add)

BufDelayC.kr(buf, in, delaytime, mul, add)

Simple delay line with cubic interpolation which uses a buffer for its internal memory. See also BufDelayN which uses no interpolation, and BufDelayL which uses linear interpolation. Cubic interpolation is more computationally expensive than linear, but more accurate.

See also DelayC.

buf - buffer number.

in - the input signal.

delaytime - delay time in seconds.

// allocate buffer

b = Buffer.alloc(s,44100,1);

(

// Dust randomly triggers Decay to create an exponential

// decay envelope for the WhiteNoise input source

{

var z = Decay.ar(Dust.ar(1,0.5), 0.3, WhiteNoise.ar);

BufDelayC.ar(b, z, 0.2, 1, z); // input is mixed with delay via the add input

}.play

)