PV_MagBelow pass bins below a threshold

PV_MagBelow(buffer, threshold)

Passes only bins whose magnitude is below a threshold.

buffer - fft buffer.

threshold - magnitude threshold.

See also FFT Overview.

s.boot;

(

b = Buffer.alloc(s,2048,1);

c = Buffer.read(s,"sounds/a11wlk01.wav");

)

(

SynthDef("help-magBelow", { arg out=0, bufnum=0;

var in, chain;

in = SinOsc.ar(SinOsc.kr(SinOsc.kr(0.08, 0, 6, 6.2).squared, 0, 100, 800));

chain = FFT(bufnum, in);

chain = PV_MagBelow(chain, 10);

Out.ar(out, 0.5 * IFFT(chain).dup);

}).play(s,[\out, 0, \bufnum, b]);

)

(

SynthDef("help-magBelow2", { arg out=0, bufnum=0;

var in, chain;

in = WhiteNoise.ar(0.2);

chain = FFT(bufnum, in);

chain = PV_MagBelow(chain, MouseX.kr(0, 7));

Out.ar(out, 0.5 * IFFT(chain).dup);

}).play(s,[\out, 0, \bufnum, b]);

)

(

SynthDef("help-magBelow3", { arg out=0, bufnum=0, soundBufnum=2;

var in, chain;

in = PlayBuf.ar(1, soundBufnum, BufRateScale.kr(soundBufnum), loop: 1);

chain = FFT(bufnum, in);

chain = PV_MagBelow(chain, MouseX.kr(0, 310));

Out.ar(out, 0.5 * IFFT(chain).dup);

}).play(s,[\out, 0, \bufnum, b, \soundBufnum, c]);

)

b.free; c.free;