BufWr buffer writing oscillator

write to a buffer at an index

see also BufRd

BufWr.ar(input, bufnum, phase, loop)

input input ugens (channelArray)

bufnum the index of the buffer to use

phase modulatable index into the buffer (has to be audio rate).

loop 1 means true, 0 means false. this is modulatable.

Note: BufWr (in difference to BufRd) does not do multichannel expansion, because input is an array.

(

// allocate a buffer for writing into

s = Server.local;

s.waitForBoot{

s.sendMsg("/b_alloc", 0, 44100 * 2);

}

)

//write into the buffer with a BufWr

(

y = { arg rate=1;

var in;

in = SinOsc.ar(LFNoise1.kr(2, 300, 400), 0, 0.1);

BufWr.ar(in, 0, Phasor.ar(0, BufRateScale.kr(0) * rate, 0, BufFrames.kr(0)));

0.0 //quiet

}.play;

)

//read it with a BufRd

(

x = { arg rate=1;

BufRd.ar(1, 0, Phasor.ar(0, BufRateScale.kr(0) * rate, 0, BufFrames.kr(0)))

}.play(s);

)

x.set(\rate, 5);

y.set(\rate, 2.0.rand);

x.set(\rate, 2);