VarSaw variable duty saw

VarSaw.ar(freq, iphase,width, mul, add)

VarSaw.kr(freq, iphase,width, mul, add)

freq - frequency in Hertz

iphase - initial phase offset in cycles ( 0..1 )

width - duty cycle from zero to one.

({

VarSaw.ar(

LFPulse.kr(#[3, 3.03], 0, 0.3, 200, 200), //freq

0, //iphase

LFTri.kr(1.0).range(0, 1), //width

0.1 //mul

)

}.play

)

({ //same but with static width

VarSaw.ar(

LFPulse.kr(#[3, 3.03], 0, 0.3, 200, 200), //freq

0, //iphase

0.2, //width

0.1 //mul

)

}.play

)

//compare:

Server.internal.boot;

({

[

LFPulse.ar(LFPulse.kr(3, 0, 0.3, 200, 200), 0, 0.2, 0.1),

VarSaw.ar(LFPulse.kr(3, 0, 0.3, 200, 200), 0, 0.2, 0.1)

]

}.scope(bufsize: 44100, zoom: 5)

)