BPF 2nd order Butterworth bandpass filter

Inherits from: Object : AbstractFunction : UGen : Filter

BPF.ar(in, freq, rq, mul, add)

BPF.kr(in, freq, rq, mul, add)

A second order Butterworth bandpass filter.

in - input signal to be processed

freq - centre frequency in Hertz.

rq - the reciprocal of Q. bandwidth / cutoffFreq.

// modulate filter frequency with a sine

{ BPF.ar(Saw.ar(200, 0.5), SinOsc.kr(XLine.kr(0.7, 300, 20), 0, 3600, 4000), 0.3) }.play;

// modulate filter frequency with the cursor position

{ BPF.ar(Saw.ar(200, 0.5), MouseX.kr(100, 10000, 1), 0.3) }.play;

// BPF on control signals:

(

{ var vib = BPF.kr(PinkNoise.kr, MouseX.kr(1, 100, 1), 0.3) * 10;

SinOsc.ar(vib * 200 + 600) * 0.2 }.play;

)