Tap A single tap into a delayline

Tap.ar(bufnum, numChannels, delaytime)

The Tap UGen allows a single tap at a delay into a buffer.

bufnum - the index of the buffer to use

numChannels - number of channels of the buffer

delaytime - tap delay; cannot be modulated

See also: PlayBuf (Tap uses the PlayBuf UGen internally).

// Create a buffer.

b=Buffer.alloc(s, s.sampleRate, 1); //enough space for one second of mono audio

// Write to the Buffer with BufWr, read using two Taps, one for each ear!

(

SynthDef(\helpTap, {|bufnum|

var source, capture;

source= SoundIn.ar(0); //use headphones to avoid feedback

capture= BufWr.ar(source, bufnum, Phasor.ar(0,1, 0, BufFrames.ir(bufnum),1));

Out.ar(0, Tap.ar(bufnum, 1, [0.1,0.9])); //multichannel expansion, so one tap each ear

}).send(s);

)

x=Synth(\helpTap,[\bufnum, b]);

x.free;