DemandEnvGen demand rate envelope generator

superclass: UGen

*ar(levels, times, shapes, curves, gate, reset, levelScale, levelOffset, timeScale, doneAction)

*kr(levels, times, shapes, curves, gate, reset, levelScale, levelOffset, timeScale, doneAction)

levels demand ugen (or other ugen) returning level values

times demand ugen (or other ugen) returning time values

shapes demand ugen (or other ugen) returning shape number - the number given is the shape number (Env)

curves demand ugen (or other ugen) returning curve values - if shape is 5, this is the curve factor

gate control rate gate

if gate is x >= 1, the ugen runs

if gate is 0 > x > 1, the ugen is released at the next level (doneAction)

if gate is x <= 0, the ugen is sampled end held

reset if reset crosses from nonpositive to positive, the ugen is reset at the next level

if it is > 1, it is reset immediately.

levelScale demand ugen returning level scaling values

levelOffset demand ugen returning level offset values

timeScale demand ugen returning time scaling values

doneAction a done action to do when one of the demand series ended (Synth-Controlling-UGens)

structurally related: EnvGen, Pseg

see also: Demand

// frequency envelope with random times

(

{

var freq;

freq = DemandEnvGen.ar(

Dseq([204, 400, 201, 502, 300, 200], inf),

Drand([1.01, 0.2, 0.1, 2], inf) * MouseY.kr(0.01, 3, 1),

7 // cubic interpolation

);

SinOsc.ar(freq * [1, 1.01]) * 0.1

}.play;

)

// frequency modulation

(

{

var freq, list;

list = { exprand(200, 1000.0) } ! 32;

freq = DemandEnvGen.ar(

{ Dseq(list.scramble, inf) } ! 2,

SampleDur.ir * MouseY.kr(1, 3000, 1),

5, // curve interpoaltion

MouseX.kr(-0.01, -4) // curve must be negative for fast interpol.

);

SinOsc.ar(freq) * 0.1

}.play;

)

// gate

// mouse x on right side of screen toggles gate

(

{

var freq;

freq = DemandEnvGen.kr(

Dwhite(300, 1000, inf).round(100),

0.1,

5, 0.3, // curve: 0.3

MouseX.kr > 0.5,

1

);

SinOsc.ar(freq * [1, 1.21]) * 0.1

}.play;

)

// sample and hold (0.5 > gate > 0)

// mouse x on right side of screen toggles gate

// mouse y scales frequency

(

{

var freq;

freq = DemandEnvGen.kr(

Dwhite(300, 1000, inf).round(100),

0.1,

5, 0.3,

MouseX.kr > 0.5 + 0.1

);

SinOsc.ar(freq * [1, 1.21]) * 0.1

}.play;

)

// gate

// mouse x on right side of screen toggles gate

// mouse button does soft reset

(

{

var freq;

freq = DemandEnvGen.kr(

Dseq([Dseries(400, 200, 5), 500, 800, 530, 4000, 900], 2),

Dseq([0.2, 0.1, 0.2, 0.3, 0.1], inf),

Dseq([1, 0, 0, 6, 1, 1, 0, 2], inf), // shapes

0,

MouseX.kr > 0.5, // gate

MouseButton.kr > 0.5, // reset

doneAction:0

);

SinOsc.ar(freq * [1, 1.001]) * 0.1

}.play;

)

// gate

// mouse x on right side of screen toggles sample and hold

// mouse button does hard reset

(

{

var freq;

freq = DemandEnvGen.kr(

Dseq([Dseries(400, 200, 5), 500, 800, 530, 4000, 900], 2),

0.1,

3, 0,

MouseX.kr > 0.5 - 0.1, // gate: sample and hold

MouseButton.kr > 0.5 * 2, // hard reset

doneAction: 0

);

SinOsc.ar(freq * [1, 1.001]) * 0.1

}.play;

)

// short sequence with doneAction, linear

(

{

var freq;

freq = DemandEnvGen.kr(

Dseq([1300, 500, 800, 300, 400], 1),

0.2,

1,

doneAction:2

);

SinOsc.ar(freq * [1, 1.01]) * 0.1

}.play;

)

// short sequence with doneAction, step

(

{

var freq;

freq = DemandEnvGen.kr(

Dseq([1300, 500, 800, 300, 400], 1),

0.2,

0,

doneAction:2

);

SinOsc.ar(freq * [1, 1.01]) * 0.1

}.play;

)

// a linear ramp

(

{

var freq;

freq = DemandEnvGen.kr(

Dseq([300, 800], 1),

1,

1

);

SinOsc.ar(freq * [1, 1.01]) * 0.1

}.play;

)

// random gate: release. gate low level > 0.

// only end points are kept as release levels

(

{

var freq;

freq = DemandEnvGen.kr(

Dseq([500, 800], inf),

0.03,

1,0, // linear

ToggleFF.kr(Dust.kr(5)) + 0.1 // gate

);

SinOsc.ar(freq * [1, 1.01]) * 0.1

}.play;

)

// random gate: sample and hold. gate low level = 0.

(

{

var freq;

freq = DemandEnvGen.kr(

Dseq([500, 800, 600], inf),

0.03,

1,0, // linear

ToggleFF.kr(Dust.kr(5)), // gate

0 // reset

);

SinOsc.ar(freq * [1, 1.01]) * 0.1

}.play;

)

// lfnoise1

(

{

DemandEnvGen.ar(

Dwhite(-0.1, 0.1, inf),

SampleDur.ir * MouseY.kr(0.5, 20),

5,

-4

);

}.play;

)

// lfbrownnoise

(

{

DemandEnvGen.ar(

Dbrown(-0.1, 0.1, 0.1, inf),

SampleDur.ir * MouseY.kr(1, 100, 1)

);

}.play;

)

Server.internal.boot;

// hardsyncing a saw

(

{

DemandEnvGen.ar(

Dseq([Dseries(-0.1, 0.01, 20)], inf),

SampleDur.ir * MouseY.kr(1, 100, 1),

1, 0,

K2A.ar(1),

Impulse.ar(MouseX.kr(1, SampleRate.ir * MouseX.kr(0.002, 1, 1), 1), 0, 1.5)

)

}.scope;

)

// softsyncing a saw

(

{

DemandEnvGen.ar(

Dseq([Dseries(-0.1, 0.01, 20)], inf),

SampleDur.ir * MouseY.kr(1, 100, 1),

1, 0,

K2A.ar(1),

Impulse.ar(MouseX.kr(1, SampleRate.ir * MouseX.kr(0.002, 1, 1), 1)) + [0, 0.3]

)

}.scope;

)

// hardsyncing a saw, som random elements

(

{

DemandEnvGen.ar(

Dseq([Dseries(-0.1, 0.01, 20), Dseries(-0.1, 0.01, 20), Dwhite(-0.1, 0.1, 5)], inf),

SampleDur.ir * MouseY.kr(1, 100, 1),

3, 0,

1,

Impulse.ar(MouseX.kr(1, SampleRate.ir * MouseX.kr(0.002, 1, 1), 1), 0, 1.5)

)

}.scope;

)

// softsyncing a saw, som random elements

(

{

DemandEnvGen.ar(

Dseq([Dseries(-0.1, 0.01, 20), Dseries(-0.1, 0.01, 20), Dwhite(-0.1, 0.1, 5)], inf),

SampleDur.ir * MouseY.kr(1, 100, 1),

1, 0, // linear interpolation

1,

Impulse.ar(MouseX.kr(1, SampleRate.ir * MouseX.kr(0.002, 1, 1), 1))

)

}.scope;

)

// multichannel expansion

// mouse x on right side of screen toggles gate

// mouse y controls speed

(

{

var freq;

freq = DemandEnvGen.kr(

{ Dseq([300, 800, Drand([1000, 460, 300], 1), 400], inf) + 3.0.rand } ! 2,

MouseY.kr(0.001, 2, 1),

5, -4,

MouseX.kr > 0.5

);

SinOsc.ar(freq) * 0.1

}.play;

)