Wrap wrap a signal outside given thresholds

Wrap.ar(in, lo, hi)

Wrap.kr(in, lo, hi)

This differs from the BinaryOpUGen wrap2 in that it allows one to set both low and high thresholds.

in - signal to be wrapped

lo - low threshold of wrapping. Must be less then hi.

hi - high threshold of wrapping. Must be greater then lo.

Server.internal.boot;

{ Wrap.ar(SinOsc.ar(440, 0, 0.2), -0.15, 0.15) }.scope;