Slew slew rate limiter

Inherits from: Object : AbstractFunction : UGen : Filter

Slew.ar(in, upSlope, downSlope, mul, add)

Slew.kr(in, upSlope, downSlope, mul, add)

Limits the slope of an input signal. The slope is expressed in units per second.

in - input signal.

upSlope - maximum upward slope.

downSlope - maximum downward slope.

(

{

z = LFPulse.ar(800);

[z, Slew.ar(z, 4000, 4000)]

}.plot)

// Has the effect of removing transients and higher frequencies.

(

{

z = Saw.ar(800, 0.2);

Slew.ar(z, 400, 400)

}.play

)