SharedOut write to a shared control bus

Inherits from: Object : AbstractFunction : UGen : AbstractOut

SharedOut.kr(bus, channelsArray)

Reads from a control bus shared between the internal server and the SC client. Control rate only. Reading from a shared control bus on the client is synchronous. When not using the internal server use the get method of Bus (or /c_get in messaging style) or SendTrig with an OSCresponder or OSCresponderNode.

bus - the index of the shared control bus to read from

channelsArray - an Array of channels or single output to write out. You cannot change the size of this once a SynthDef has been built.

(

// only works with the internal server

s = Server.internal;

s.boot;

)

(

SynthDef("help-SharedOut", {

SharedOut.kr(0, SinOsc.kr(0.2));

}).send(s);

)

(

s.sendMsg(\s_new, "help-SharedOut", x = s.nextNodeID, 0, 1);

s.sendMsg(\n_trace, x);

// poll the shared control bus

Routine({

30.do({

s.getSharedControl(0).postln;

0.2.wait;

});

}).play;

)

s.quit;