LeakDC remove DC offset

Inherits from: Object : AbstractFunction : UGen : Filter

LeakDC.ar(in, coef, mul, add)

LeakDC.kr(in, coef, mul, add)

This filter removes a DC offset from a signal.

in - input signal.

coef - leak coefficient. Defaults to 0.995 for audiorate and 0.9 for controlrate.

Server.internal.boot;

(

{

var a;

a = LFPulse.ar(800, 0.5, 0.5, 0.5);

[a, LeakDC.ar(a, 0.995)]

}.scope(bufsize: 22050)

)